PU2CLR RDA5807 Arduino Library 1.0.1 Arduino Library for RDA5807 Devices - By Ricardo Lima Caratti

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - b -

- blockB : rds_blockb

### - c -

- clearRdsFifo() : RDA5807
- clockType : RDA5807
- currentFMBand : RDA5807
- currentFMSpace : RDA5807
- currentFrequency : RDA5807
- currentVolume : RDA5807

### - d -

- deviceAddressDirectAccess : RDA5807
- deviceAddressFullAccess : RDA5807

### - g -

- getBlockId() : RDA5807
- getDeviceId() : RDA5807
- getErrorBlockB() : RDA5807
- getFrequency() : RDA5807
- getNext2Block() : RDA5807
- getNext4Block() : RDA5807
- getRdsFlagAB() : RDA5807
- getRdsGroupType() : RDA5807
- getRdsProgramType() : RDA5807
- getRdsReady() : RDA5807
- getRdsSync() : RDA5807
- getRdsText() : RDA5807
- getRdsText0A() : RDA5807
- getRdsText2A() : RDA5807
- getRdsText2B() : RDA5807
- getRdsTime() : RDA5807
- getRdsVersionCode() : RDA5807
- getRealChannel() : RDA5807
- getRealFrequency() : RDA5807
- getRssi() : RDA5807
- getStatus() : RDA5807
- getStatusRegisters() : RDA5807
- getVolume() : RDA5807
- gpio1Control : RDA5807
- gpio2Control : RDA5807
- gpio3Control : RDA5807
- group0 : rds_blockb
- group2 : rds_blockb

### - h -

- hasRdsInfo() : RDA5807

### - i -

- isStereo() : RDA5807

### - m -

- maxDelayAftarCrystalOn : RDA5807

### - o -

- oscillatorType : RDA5807

### - p -

- powerDown() : RDA5807
- powerUp() : RDA5807

### - r -

- raw : rda_reg00 , rda_reg01 , rda_reg02 , rda_reg03 , rda_reg04 , rda_reg05 , rda_reg06 , rda_reg07 , rda_reg08 , rda_reg0a , rda_reg0b , rds_date_time , word16_to_bytes
- RDSA : rda_reg0c
- RDSB : rda_reg0d
- RDSC : rda_reg0e
- RDSD : rda_reg0f
- refined : rda_reg00 , rda_reg01 , rda_reg02 , rda_reg03 , rda_reg04 , rda_reg05 , rda_reg06 , rda_reg07 , rda_reg08 , rda_reg0a , rda_reg0b , rda_reg0c , rda_reg0d , rda_reg0e , rda_reg0f , rds_blockb , rds_date_time , word16_to_bytes
- resetPin : RDA5807

### - s -

- seek() : RDA5807
- setBand() : RDA5807
- setBass() : RDA5807
- setChannel() : RDA5807
- setDelayAfterCrystalOn() : RDA5807
- setFmDeemphasis() : RDA5807
- setFrequency() : RDA5807
- setFrequencyDown() : RDA5807
- setFrequencyUp() : RDA5807
- setGpio() : RDA5807
- setI2CBusAddrs() : RDA5807
- setMono() : RDA5807
- setMute() : RDA5807
- setRBDS() : RDA5807
- setRDS() : RDA5807
- setRdsFifo() : RDA5807
- setRegister() : RDA5807
- setSeekThreshold() : RDA5807
- setSoftmute() : RDA5807
- setSpace() : RDA5807
- setup() : RDA5807
- setVolume() : RDA5807
- setVolumeDown() : RDA5807
- setVolumeUp() : RDA5807
- softReset() : RDA5807

### - w -

- waitAndFinishTune() : RDA5807